OE57HSG  Gearbox Stepping Motor/57mm混合式步进齿轮电机 

基本性能/General Specification:

	内齿圈材料         Housing Material
	金属      Metal

	输出轴轴承形式     Bearing at Output
	滚动轴承  Ball Bearings

	最大允许径向负载（离法兰12mm处）Max.Radial Load(12mm from flange)
	 ≤180N

	最大允许轴向负载Max.Shaft Axial Load
	≤30N


                                           

	型号

Model No.
	步距角

Step Angle
	长度

Motor Length
	电流

Current

/Phase
	电阻

Resistance

/Phase
	电感

Inductance

/Phase
	静转矩

Holding Torque
	引线数

# of Leads
	定位转矩

Detent Torque
	转子惯量

Rotor Inertia
	重量

Mass

	
	( °)
	(L1)mm
	A
	Ω
	mH
	N.m
	No.
	g.cm
	g.cm
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	Kg

	OE57HS41-2804
	1.8
	41
	2.8
	0.7
	1.4
	0.55
	4
	250
	150
	0.47

	OE57HS51-2804
	1.8
	51
	2.8
	0.83
	2.2
	1.01
	4
	300
	230
	0.59

	OE57HS56-2804
	1.8
	56
	2.8
	0.9
	2.5
	1.2
	4
	350
	280
	0.68

	OE57HS64-2804
	1.8
	64
	2.8
	0.8
	2.3
	1
	4
	400
	300
	0.75

	OE57HS76-2804
	1.8
	76
	2.8
	1.1
	3.6
	1.89
	4
	600
	440
	1.1

	OE57HS82-3004
	1.8
	82
	3
	1.2
	4
	2.1
	4
	1000
	600
	1.2

	OE57HS100-4204
	1.8
	100
	4.2
	0.75
	3
	3
	4
	1100
	700
	1.3

	OE57HS112-4204
	1.8
	112
	4.2
	0.9
	3.8
	3.1
	4
	1200
	800
	1.4


以上仅为代表产品，特殊产品可根据客户要求订制。

Above only for representative products, products of special request can be made according to the customer request.
偏心减速箱规格/Gearbox Specification:

	减速比Reduction ratio
	3
	7.5
	12.5
	15
	25
	30
	50
	75
	90
	100
	120
	150

	减速级数Number of gear trains
	2
	3
	4
	5

	减速箱长度(L2)Length(mm)
	32&42
	42

	峰值力距Peak torque(kg.cm)
	50

	空载间隙 Backlash at Noload(度)
	4 deg
	3.5deg
	3deg
	2.5deg


电机外型图/Dimensions:(单位/Unit=mm)             接线图/Wiring Diagram:
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电机规格/Electrical Specification: 
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