1.8° 28mm两相混合式步进丝杆电机 28mm 2phase hybrid screw rod stepper motor

基本性能/General Specification:

电机规格/Electrical Specification:   

	型号

Model No.
	步距角

Step Angle
	长度

Motor Length
	电流

Current

/Phase
	电阻

Resistance

/Phase
	电感

Inductance

/Phase
	静转矩

Holding Torque
	引线数

# of Leads
	转子惯量

Rotor Inertia
	重量

Motor

Weight 

	
	( °)
	(L)mm
	A
	Ω
	mH
	g.cm
	No.
	g.cm
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	Kg

	OE28HS32-0424
	1.8
	32
	0.4
	11.9
	6.7
	600
	4
	9
	0.11

	OE28HS32-0504
	1.8
	32
	0.5
	11.4
	7.4
	600
	4
	9
	0.11

	OE28HS32-0674
	1.8
	32
	0.67
	5.6
	3.4
	600
	4
	9
	0.11

	OE28HS45-0674
	1.8
	45
	0.67
	6.8
	4.9
	950
	4
	12
	0.14

	OE28HS51-0674
	1.8
	51
	0.67
	9.2
	7.2
	1200
	4
	18
	0.2

	OE28HS51-1004
	1.8
	51
	1.0
	2.3
	1.8
	900
	4
	18
	0.2


以上仅为代表产品，特殊产品可根据客户要求订制。

Above only for representative products, products of special request can be made according to the customer request.
丝杆规格/Screw rod Specification:

	丝杆直径

Screw Diameter(mm)
	丝杆导程

Screw Lead(mm)     
	丝杆螺距

Screw Pitch(mm)
	步长

Travel per step(mm)
	丝杆直径

Screw Diameter(mm)
	丝杆导程

Screw Lead(mm)     
	丝杆螺距

Screw Pitch(mm)
	步长

Travel per step(mm)

	Tr3.5
	1
	1
	0.005
	Tr6
	2
	1
	0.01

	
	0.6096
	0.6096
	0.003
	
	4
	1
	0.02

	
	2.4384
	1.2192
	0.0122
	
	6
	1
	0.03

	Tr5
	1
	1
	0.005
	
	12
	2
	0.06

	
	2
	1
	0.01
	
	
	
	


电机外型图/Dimensions:(单位/Unit=mm)           

  螺母/Nut: 1.POM螺母/POM Nut

                                                                 2.铜螺母/Copper Nut
1、External Shaft motor
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2、Non Captive motor
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接线图/Wiring Diagram:
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项目(Item)�
性能(Specifications)�
�
�
步距角(Step Angle)�
1.8°�
�
�
温  升(Temperature Rise)�
80℃max�
�
�
环境温度(Ambient Temperature）�
-20℃~+50℃�
�
�
绝缘电阻(Insulation Resistance)�
100 MΩ Min. ,500VDC�
�
�
电气强度(Dielectric Strength):�
500VAC for 1minute �
�
�
径向间隙(Shaft Radial Play)�
0.02Max. (450g-load)�
�
�
轴向间隙(Shaft Axial Play)�
0.08Max. (450g-load)�
�
�
最大径向压力(Max. radial force)�
28N (20mm from the flange)�
�
�
最大轴向压力(Max. axial force)�
10N�
�
�
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