1.8° 42mm两相混合式步进丝杆电机 42mm 2phase hybrid screw rod stepper motor

基本性能/General Specification:

电机规格/Electrical Specification:                                             

	型号

Model No.
	步距角

Step Angle
	长度

Motor Length
	电流

Current

/Phase
	电阻

Resistance

/Phase
	电感

Inductance

/Phase
	静转矩

Holding Torque
	引线数

# of Leads
	定位转矩

Detent Torque
	转子惯量

Rotor Inertia
	重量

Mass

	
	( °)
	(L)mm
	A
	Ω
	mH
	N.m
	No.
	g.cm
	g.cm
[image: image1.wmf]2


	Kg

	OE42HS25-0404
	1.8
	25
	0.4
	24
	36
	1.8
	4
	75
	20
	0.15

	OE42HS34-1334
	1.8
	34
	1.33
	2.1
	2.5
	2.2
	4
	120
	34
	0.22

	OE42HS40-1684
	1.8
	40
	1.68
	1.65
	3.2
	3.6
	4
	150
	54
	0.28

	OE42HS48-1684
	1.8
	48
	1.68
	1.65
	2.8
	4.4
	4
	260
	68
	0.35

	OE42HS60-1004
	1.8
	60
	1.0
	8
	13
	7.5
	4
	280
	102
	0.5


以上仅为代表产品，特殊产品可根据客户要求订制。

Above only for representative products, products of special request can be made according to the customer request.
丝杆规格/Screw rod Specification:

	丝杆直径

Screw Diameter(mm)
	丝杆导程

Screw Lead(mm)     
	丝杆螺距

Screw Pitch(mm)
	步长

Travel per step(mm)
	丝杆直径

Screw Diameter(mm)
	丝杆导程

Screw Lead(mm)     
	丝杆螺距

Screw Pitch(mm)
	步长

Travel per step(mm)

	Tr5
	1
	1
	0.005
	Tr8
	8
	2
	0.04

	
	2
	1
	0.01
	
	10
	2
	0.05

	Tr6
	2
	1
	0.01
	
	12
	2
	0.06

	
	4
	1
	0.02
	
	14
	2
	0.07

	
	6
	1
	0.03
	Tr10
	2
	2
	0.01

	
	12
	2
	0.06
	
	3
	1.5
	0.015

	Tr8
	1
	1
	0.005
	
	4
	2
	0.02

	
	2
	2
	0.01
	
	8
	2
	0.04

	
	3
	1.5
	0.015
	
	10
	2
	0.05

	
	4
	2
	0.02
	
	12
	2
	0.06


电机外型图/Dimensions:(单位/Unit=mm)              

螺母/Nut: 1.POM螺母/POM Nut

                                                           2.铜螺母/Copper Nut
1、External Shaft motor
[image: image2.png]AutoCAD 2007 - [EASSEE\SE eI EHR\A2HSAEH\40LE\42HS40-1704T18-30 #HEH dwa] (=2 =R
@ NEE

B¥xax| 9

L2+1 L1+1 42.3Max.

2 31+0.1
R

3110.1
42.3Max.

’(V\ .
a \é ;_< !
g) 4-M3*0.5
@© Deep4.5Min.
= £
E !
26AWG e
UL1007 "

CERECACIAL: =) £
FRERDREH B ERELGTRRD 1R ESC o ENIER RBL, RESTRITERETRENS.

& E H\‘ © H\‘ e H Al H ‘ - oo




       [image: image3.png]AutoCAD 2007 - [EASHEE\SEFEHIE\A2HS\HIHE-H\406L5\42HS40- 1704TL8-30 HIHEH.dwg] o=@ =

&l¥xax|o

5

Traxs(

022
?10

1

CERECACIAL: =) £
FRERDREH B ERELGTRRD 1R ESC o ENIER RBL, RESTRITERETRENS.

5 ERERER] - e





2、Non Captive motor
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接线图/Wiring Diagram:
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项目(Item)�
性能(Specifications)�
�
�
步距角(Step Angle)�
1.8°�
�
�
温  升(Temperature Rise)�
80℃max�
�
�
环境温度(Ambient Temperature）�
-20℃~+50℃�
�
�
绝缘电阻(Insulation Resistance)�
100 MΩ Min. ,500VDC�
�
�
电气强度(Dielectric Strength):�
500VAC for 1minute �
�
�
径向间隙(Shaft Radial Play)�
0.02Max. (450g-load)�
�
�
轴向间隙(Shaft Axial Play)�
0.08Max. (450g-load)�
�
�
最大径向压力(Max. radial force)�
28N (20mm from the flange)�
�
�
最大轴向压力(Max. axial force)�
10N�
�
�
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