1.8° 57mm两相混合式步进丝杆电机 57mm 2phase hybrid screw rod stepper motor

基本性能/General Specification:

电机规格/Electrical Specification:                                             

	型号

Model No.
	步距角

Step Angle
	长度

Motor Length
	电流

Current

/Phase
	电阻

Resistance

/Phase
	电感

Inductance

/Phase
	静转矩

Holding Torque
	引线数

# of Leads
	定位转矩

Detent Torque
	转子惯量

Rotor Inertia
	重量

Mass

	
	( °)
	(L)mm
	A
	Ω
	mH
	N.m
	No.
	g.cm
	g.cm
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	Kg

	OE57HS41-2804
	1.8
	41
	2.8
	0.7
	1.4
	0.55
	4
	250
	150
	0.47

	OE57HS51-2804
	1.8
	51
	2.8
	0.83
	2.2
	1.01
	4
	300
	230
	0.59

	OE57HS56-2804
	1.8
	56
	2.8
	0.9
	2.5
	1.2
	4
	350
	280
	0.68

	OE57HS64-2804
	1.8
	64
	2.8
	0.8
	2.3
	1
	4
	400
	300
	0.75

	OE57HS76-2804
	1.8
	76
	2.8
	1.1
	3.6
	1.89
	4
	600
	440
	1.1

	OE57HS82-3004
	1.8
	82
	3
	1.2
	4
	2.1
	4
	1000
	600
	1.2

	OE57HS100-4204
	1.8
	100
	4.2
	0.75
	3
	3
	4
	1100
	700
	1.3

	OE57HS112-4204
	1.8
	112
	4.2
	0.9
	3.8
	3.1
	4
	1200
	800
	1.4


以上仅为代表产品，特殊产品可根据客户要求订制。

Above only for representative products, products of special request can be made according to the customer request.

丝杆规格/Screw rod Specification:

	丝杆直径

Screw Diameter(mm)
	丝杆导程

Screw Lead(mm)     
	丝杆螺距

Screw Pitch(mm)
	步长

Travel per step(mm)
	丝杆直径

Screw Diameter(mm)
	丝杆导程

Screw Lead(mm)     
	丝杆螺距

Screw Pitch(mm)
	步长

Travel per step(mm)

	Tr8


	1
	1
	0.005
	Tr8


	10
	2
	0.05

	
	2
	2
	0.01
	
	12
	2
	0.06

	
	3
	1.5
	0.015
	
	14
	2
	0.07

	
	4
	2
	0.02
	
	
	
	

	
	8
	2
	0.04
	
	
	
	

	丝杆直径

Screw Diameter(mm)
	丝杆导程

Screw Lead(mm)     
	丝杆螺距

Screw Pitch(mm)
	步长

Travel per step(mm)
	丝杆直径

Screw Diameter(mm)
	丝杆导程

Screw Lead(mm)     
	丝杆螺距

Screw Pitch(mm)
	步长

Travel per step(mm)

	Tr10
	2
	2
	0.01
	Tr12

	2
	2
	0.01

	
	3
	1.5
	0.015
	
	3
	3
	0.015

	
	4
	2
	0.02
	
	8
	2
	0.04

	
	8
	2
	0.04
	
	10
	2
	0.05

	
	10
	2
	0.05
	
	
	
	

	
	12
	2
	0.06
	
	
	
	


电机外型图/Dimensions:(单位/Unit=mm)
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接线图/Wiring Diagram:
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项目(Item)�
性能(Specifications)�
�
�
步距角(Step Angle)�
1.8°�
�
�
温  升(Temperature Rise)�
80℃max�
�
�
环境温度（Ambient Temperature）�
-20℃~+50℃�
�
�
绝缘电阻(Insulation Resistance)�
100 MΩ Min. ,500VDC�
�
�
电气强度(Dielectric Strength):�
500VAC for 1minute �
�
�
径向间隙(Shaft Radial Play)�
0.02Max. (450g-load)�
�
�
轴向间隙(Shaft Axial Play)�
0.08Max. (450g-load)�
�
�
最大径向压力(Max. radial force)�
75N (20mm from the flange)�
�
�
最大轴向压力(Max. axial force)�
15N�
�
�
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