1.8° 86mm两相混合式步进丝杆电机 86mm 2phase hybrid screw rod stepper motor

基本性能/General Specification:

电机规格/Electrical Specification:  

	型号

Model No.
	步距角

Step Angle
	长度

Motor Length
	电流

Current

/Phase
	电阻

Resistance

/Phase
	电感

Inductance

/Phase
	静转矩

Holding Torque
	引线数

# of Leads
	定位转矩

Detent Torque
	转子惯量

Rotor Inertia
	重量

Mass

	
	( °)
	(L)mm
	A
	Ω
	mH
	N.m
	No.
	Kg.cm
	g.cm
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	Kg

	OE86HS78-5504
	1.8
	78
	5.5
	0.46
	4.0
	4.6
	4
	1.2
	1400
	2.3

	OE86HS78-4208
	1.8
	78
	4.2
	0.75
	3.4
	3.2
	8
	1.2
	1400
	2.3

	OE86HS97-6004
	1.8
	97
	6.0
	0.5
	3.8
	7.0
	4
	1.7
	2100
	3.0

	OE86HS115-6004
	1.8
	115
	6.0
	0.5
	5.8
	8.7
	4
	2.4
	2700
	3.8

	OE86HS155-6004
	1.8
	155
	6.0
	0.68
	9.0
	13
	4
	3.6
	4000
	5.4

	OE86HS155-4208
	1.8
	155
	4.2
	1.25
	8.0
	8.5
	8
	3.6
	4000
	5.4


以上仅为代表产品，特殊产品可根据客户要求订制。

Above only for representative products, products of special request can be made according to the customer request.
丝杆规格/Screw rod Specification:

	丝杆直径

Screw Diameter(mm)
	丝杆导程

Screw Lead(mm)     
	丝杆螺距

Screw Pitch(mm)
	步长

Travel per step(mm)
	丝杆直径

Screw Diameter(mm)
	丝杆导程

Screw Lead(mm)     
	丝杆螺距

Screw Pitch(mm)
	步长

Travel per step(mm)

	Tr10
	2
	2
	0.01
	Tr12

	2
	2
	0.01

	
	3
	1.5
	0.015
	
	3
	3
	0.015

	
	4
	2
	0.02
	
	8
	2
	0.04

	
	8
	2
	0.04
	
	10
	2
	0.05

	
	10
	2
	0.05
	
	
	
	

	
	12
	2
	0.06
	
	
	
	


电机外型图/Dimensions:(单位/Unit=mm)                                                                                
1、External Shaft motor
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2、Non Captive motor
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接线图/Wiring Diagram:
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项目(Item)�
性能(Specifications)�
�
�
步距角(Step Angle)�
1.8°�
�
�
温  升(Temperature Rise)�
80℃max�
�
�
环境温度（Ambient Temperature）�
-20℃~+50℃�
�
�
绝缘电阻(Insulation Resistance)�
100 MΩ Min. ,500VDC�
�
�
电气强度(Dielectric Strength):�
820VAC for 1s 3mA�
�
�
径向间隙(Shaft Radial Play)�
0.02Max. (450g-load)�
�
�
轴向间隙(Shaft Axial Play)�
0.08Max. (450g-load)�
�
�
最大径向压力(Max. radial force)�
220N (20mm from the flange)�
�
�
最大轴向压力(Max. axial force)�
60N�
�
�
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