1.8°60mm两相混合式伺服步进电机 1.8°60mm(NEMA24) 2 phase servo stepper motor
	项目(Item)
	性能(Specifications)
	

	步距角(Step Angle)
	1.8°
	

	温  升(Temperature Rise)
	80℃max
	

	环境温度（Ambient Temperature）
	-20℃~+50℃
	

	绝缘电阻(Insulation Resistance)
	100 MΩ Min. ,500VDC
	

	电气强度(Dielectric Strength):
	500VAC for 1s 3mA
	

	径向间隙(Shaft Radial Play)
	0.02Max. (450g-load)
	

	轴向间隙(Shaft Axial Play)
	0.08Max. (450g-load)
	

	最大径向压力(Max. radial force)
	75N (20mm from the flange)
	

	最大轴向压力(Max. axial force)
	15N
	


基本性能/Genaral Specification:

电机规格/Electrical Specification:

	型号

Model No.
	步距角

Step Angle
	长度

Motor Length
	电流

Current

/Phase
	电阻

Resistance

/Phase
	电感

Inductance

/Phase
	静转矩

Holding Torque
	引线数

# of Leads
	定位转矩

Detent Torque
	转子惯量

Rotor Inertia
	重量

Mass

	
	( °)
	(L)mm
	A
	Ω
	mH
	N.m
	No.
	Kg.cm
	g.cm
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	Kg

	OE60HS88-4004BFED-0.35M
	1.8
	88
	4.0
	0.65
	2.4
	3.1
	4
	1000
	840
	1.4

	OE60HS100-4004BFED-0.35M
	1.8
	100
	4.0
	0.7
	3.0
	4.0
	4
	1100
	980
	2.0


以上仅为代表产品，特殊产品可根据客户要求订制。

Above only for representative products, products of special request can be made according to the customer request.
Dimensions:(电机外型图)

(Unit=mm)
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Wiring Diagram:(接线图)
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Motor Wiring Diagram: Encoder Wiring Diagram:
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